{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Table 5-1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Table 5-1","index":0,"n_rows":13,"n_cols":26,"rows_kept":13,"cut":false,"hidden":false,"merged":[[7,26,8,26],[7,27,8,27],[7,28,8,28],[7,21,8,21],[7,22,8,22],[7,23,8,23],[7,24,8,24],[7,25,8,25],[7,16,8,16],[7,17,8,17],[7,18,8,18],[7,19,8,19],[7,20,8,20],[7,11,8,11],[7,12,8,12],[7,13,8,13],[7,14,8,14],[7,15,8,15],[7,5,8,5],[7,6,8,6],[7,7,8,7],[7,8,8,8],[7,9,8,9],[7,0,8,0],[7,1,8,1],[7,2,8,2],[7,3,8,3],[7,4,8,4],[2,1,2,25],[1,1,1,25],[3,23,4,25],[6,1,6,13],[4,17,4,18],[4,19,4,20],[3,17,3,20],[3,4,4,7],[6,15,6,25]]}
[]
[]
[null,"Table 5-1. Proposed List of Projects and Management Actions"]
[null,null,null,null,"Relevant Sustainability Indicators Affected",null,null,null,null,null,null,null,null,null,null,null,null,"Expected Benefits",null,null,null,null,null,"Estimated Costs"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Primary ",null,"Secondary"]
[null,"MA Number","MA Name","Summary Description","Goundwater Levels and Storage","Goundwater Quality","Land Subsidence","Sw & GW Interconnection","Cirumstance for Implementation","Public Noticing Process","Permitting and Regulatory Process Requirements","Implementing YSGA Member Agency","Status","Timetable / Circumstances for Initiation",null,"Timetable for Completion","Timetable for Accural of Expected Benefits","Water Supply Augmentation","Water Demand Reduction","Water Quality Improvement","Water Management Flexibility / Efficiency","Source(s) of Water, if Applicable","Legal Authority Required","One-time Costs","Ongoing Costs (per year)","Potential Funding Source(s)"]
[]
[null,"Example 1","Enhanced Groundwater Recharge ","Development of surface and subsurface recharge projects underlying developed agricultural lands to increase groundwater recharge capacity ","•",null,null,null,"Upon adoption of Yolo GSP","Yolo GSA Board Meetings & Website  ","Site specific","YSGA","Ongoing ",2020,null,2040,"During above average water alloaction years","Up to 20,000 af average annual",null,"•","•",null,"District authorities","TBD",25000,"District"]
[null,null,null,null,null,null,null,null,null,null,"(CEQA)"]
[null,"Example 2","Cache Creek MAR","Development of floodwater capture and recharge program ffrom Poso Creek flood flows ","•",null,"•",null,"Upon completion of feasibility and permitting requirements","Yolo GSA Board Meetings & Website  ","CEQA","YSGA","Undergoing pre-feasibility analysis",2020,null,2028,"Wet year following project completion","1,200 af average annual",null,null,null,"Cache Creek","District authorities","TBD","TBD","District"]
[null,1]
[null,{"$f":"B11+1","v":2}]
[null,{"$f":"B12+1","v":3}]